# submixer4x2.dsp

Four-channel stereo submixer.

### Function

This is a four-channel stereo mixer. The total gain on a side should not exceed $7FFF. The output is available directly and can be used as an input to other instruments. This could be used to mix signals before being passed to an effects processor.

### Knobs

LeftGain0 - 0 -> $7FFF

LeftGain1 - 0 -> $7FFF

LeftGain2 - 0 -> $7FFF

LeftGain3 - 0 -> $7FFF

RightGain0 - 0 -> $7FFF

RightGain1 - 0 -> $7FFF

RightGain2 - 0 -> $7FFF

RightGain3 - 0 -> $7FFF

### Inputs

Input0

Input1

Input2

Input3

### Outputs

Left Output

Right Output

### Input FIFOs

None

### Output FIFOs

None

### Resources

Ticks = 32

N memory = 32 words