# timesplus.dsp

Mix control signals.

### Function

This instrument is the A*B+C modulator, which is useful for mixing control signals. The result is clipped to -$8000 and +$7FFF, the range of signed values. This limits its usefulness with sample players that use unsigned frequency between 0 and $FFFF.

### Notes

Multiplying 0x8000 by 0x8000 causes an overflow yielding a result of 0x8000. This means that (-1) x (-1) = (-1). Thus, if you multiply a signal by 0x8000, it will pop if the signal also contains 0x8000.

### Knobs

InputA

InputB

InputC

### Inputs

None

### Outputs

Output

### Input FIFOs

None

### Output FIFOs

None

### Resources

Ticks = 10

N memory = 7 words