# halfstereosample.dsp

Play a stereophonic sample at 22050 Hertz.

### Function

This instrument plays a stereophonic sample at 22050 Hertz.

### Knobs

Amplitude - 0 => $7FFF

### Inputs

None

### Outputs

LeftOutput

RightOutput

### Input FIFOS

InFIFO

### Output FIFOS

None

### Resources

Ticks = 36

N memory = 44 words

### Notes

The left/right channels are likely to be reversed from what you expect due to an unexpected hardware/software interaction. Please test the stereo output carefully, if this matters, and reconnect the outputs of this instrument appropriately. Only 16-bit stereo players are effected by this.