delaystero.dsp

# delaystereo.dsp

Write stereo input to an output FIFO.

### Function

This instrument writes input to an output FIFO. It is used as a building block for reverberation and echo effects. It can only write to special samples created using `CreateDelayLine()`.

### Knobs

None

### Inputs

InputLeft

InputRight

### Outputs

None

### Input FIFOs

None

### Output FIFOs

OutFIFO

### Resource

Ticks = 12

N memory = 10 words