# submixer8x2.dsp

Eight-channel stereo submixer.

### Function

This is an eight-channel stereo mixer. The total gain on a side should not exceed $7FFF. Output is available directly and can be used as an input to other instruments. It could be used to mix signals before being passed to an effects processor.

### Knobs

LeftGain0 - 0 -> $7FFF

LeftGain1 - 0 -> $7FFF

...and so on up to...

LeftGain6 - 0 -> $7FFF

LeftGain7 - 0 -> $7FFF

RightGain0 - 0 -> $7FFF

RightGain1 - 0 -> $7FFF

...and so on up to...

RightGain6 - 0 -> $7FFF

RightGain7 - 0 -> $7FFF

### Inputs

Input0

Input1

...and so on up to...

Input6

Input7

### Outputs

LeftOutput

RightOutput

### Input FIFOs

None

### Output FIFOs

None

### Resources

Ticks = 56

N memory = 56 words