# minimum.dsp

Pick the minimum of two input signals.

### Function

Outputs the smaller of InputA and InputB. This can be used for clipping.

By connecting Output to InputB, you can measure a historical minimum. In this configuration, `StartInstrument()` can be used to reset the historical maximum.

Input values are signed as usual.

### Knobs

InputA

InputB

### Outputs

Output
  MIN(InputA,InputB)

### Resources

Ticks: 12

Code: 11 words

### Implementation

V24

### See Also

``maximum.dsp`, add.dsp`