# fixedstereosample.dsp

Play a stereophonic sample at 44,100 hertz.

### Function

This instrument plays a stereophonic sample at a 44,100 hertz.

### Knobs

Amplitude - 0 => $7FFF

### Inputs

None

### Outputs

LeftOutput

RightOutput

### Input FIFOs

InFIFO

### Output FIFOs

None

### Resources

Ticks = 18

N memory = 16 words

### Notes

The left/right channels are likely to be reversed from what you expect due to an unexpected hardware/software interaction. Please test the stereo output carefully, if this matters, and reconnect the outputs of this instrument appropriately. Only 16-bit stereo players are effected by this.