# mixer8x2amp.dsp

Eight channel stereo mixer with master gain.

### Function

This is an eight channel stereo mixer. The total gain on a side should not exceed $7FFF. The output is added to the output of the other mixers, then sent to the DAC by head.dsp. This mixer has an additional master gain control that can be used to fade control the entire mix.

### Knobs

LeftGain0 - 0 -> $7FFF

LeftGain1 - 0 -> $7FFF

...and so on up to...

LeftGain6 - 0 -> $7FFF

LeftGain7 - 0 -> $7FFF

RightGain0 - 0 -> $7FFF

RightGain1 - 0 -> $7FFF

...and so on up to...

RightGain6 - 0 -> $7FFF

RightGain7 - 0 -> $7FFF

Amplitude - 0 -> $7FFF, default $7FFF = master gain control

### Inputs

Input0

Input1

...and so on up to...

Input6

Input7

### Outputs

None

### Input FIFOs

None

### Output FIFOs

None

### Resources

Ticks = 61

N memory = 59 words