submixer.dsp

# submixer2x2.dsp

Two channel stereo submixer.

### Function

This is a four channel stereo mixer. The total gain on a side should not exceed $7FFF. The output is available directly and can be used as an input to other instruments. This could be used to mix signals before being passed to an effects processor.

### Knobs

LeftGain0 - 0 -> $7FFF

LeftGain1 - 0 -> $7FFF

RightGain0 - 0 -> $7FFF

RightGain1 - 0 -> $7FFF

### Inputs

Input0

Input1

### Outputs

LeftOutput

RightOutput

### Input FIFOs

None

### Output FIFOs

None

### Resources

Ticks = 20

N memory = 20 words