# mixer4x2.dsp

Four-channel stereo mixer.

### Function

This is a four-channel stereo mixer. The total gain on a side should not exceed $7FFF. Its output is added to the output of the other mixers, then sent to the DAC by head.dsp.

### Knobs

LeftGain0 - 0 -> $7FFF

LeftGain - 0 -> $7FFF

LeftGain2 - 0 -> $7FFF

LeftGain3 - 0 -> $7FFF

RightGain0 - 0 -> $7FFF

RightGain1 - 0 -> $7FFF

RightGain2 - 0 -> $7FFF

RightGain3 - 0 -> $7FFF

### Inputs

Input0

Input1

Input2

Input3

### Outputs

None

### Input FIFOs

None

### Output FIFOs

None

### Resources

Ticks = 32

N memory = 32 words