# mixer8x2.dsp

Eight-channel stereo mixer.

### Function

This is an eight-channel stereo mixer. The total gain on a side should not exceed $7FFF. Its output is added to the output of the other mixers, then sent to the DAC by head.dsp.

### Knobs

LeftGain0 - 0 -> $7FFF

LeftGain1 - 0 -> $7FFF

...and so on up to...

LeftGain6 - 0 -> $7FFF

LeftGain7" - 0 -> $7FFF

RightGain0 - 0 -> $7FFF

RightGain1 - 0 -> $7FFF

...and so on up to...

RightGain6 - 0 -> $7FFF

RightGain7 - 0 -> $7FFF

### Inputs

Input0

Input1

...and so on up to...

Input6

Input7

### Outputs

None

### Input FIFOs

None

### Output FIFOs

None

### Resources

Ticks = 56

N memory = 56 words