# MapAACelToCQuad

Maps an anti-aliased cel to a quad.

### Synopsis

`void MapAACelToCQuad (CCB *aacel, CQuad *quad)`

### Description

Maps an anti-aliased cel to a specified quad. It is effectively a standard `MapCel()` call that stores its results into both the data and alpha-channel CCBs. It also works correctly if aacel points to a single standalone cel.

### Arguments

aacel
  Pointer to the cel to be mapped.

quad
  Pointer to the CQuad to which the cel is to be mapped.

### Implementation

Library call implemented in lib3do.lib.

### Associated Files

lib3do.lib, celutils.h

### See Also

``MapCelToCQuad`, MapCelListToCQuad`