sawfilderedsaw.dsp

# sawfilteredsaw.dsp

Filtered sawtooth with sawtooth modulation.

### Function

This instrument passes a sawtooth wave through the state variable filter. The filter cutoff frequency is modulated with another sawtooth instrument. Try setting the Resonance to 0-10, SawAmpl = 0-40.

### Knobs

Amplitude - 0 => $7FFF, final amplitude of voice

Frequency - 0 => $2000, default $100. Non-linear cutoff frequency of filter.

Resonance - 1 / Q, 0 => $6000, default $1000 = filter will ring at low values.

LFORate - 0 => $0100, default $0020, rate of sawtooth modulating filter

LFODepth - 0 => $2000, default $0100, Amplitude of sawtooth modulating filter. Actual cutoff is = Frequency + SawtoothOutput*LFODepth.

Sawtooth - 0 => $0400, default = $0100 = frequency of primary sawtooth.

SawAmplitude - 0 => $7FFF, default = $7FFF = amplitude of primary sawtooth.

### Inputs

None

### Outputs

Output

### Input FIFOs

None

### Output FIFOs

None

### Resource

Ticks = 35

N memory = 35 words